Excavator Service Schedule

|  |  |
| --- | --- |
| Make: | Model: |
| ID #: | Model Year: |
| SIN: |  |

|  |  |  |  |
| --- | --- | --- | --- |
| Done | Not Done |  | Notes and Comments |
|  |  | 120 Hours |  |
|  |  | Check travel reduction unit oil |  |
|  |  | Check swing reduction oil |  |
|  |  | 250 Hours |  |
|  |  | Drain hydraulic oil tank |  |
|  |  | Drain fuel tank |  |
|  |  | Lubricate bucket grease fittings |  |
|  |  | Clean cab outside air filter |  |
|  |  | Check track tension |  |
|  |  | 500 Hours |  |
|  |  | Clean cab air recirculation filter |  |
|  |  | Replace engine oil and filter |  |
|  |  | Replace fuel filter |  |
|  |  | Replace fuel pre-filter |  |
|  |  | Grease swing bearing |  |
|  |  | Lubricate boom lift |  |
|  |  | 1000 Hours |  |
|  |  | Replace engine air filters |  |
|  |  | Replace hydraulic oil return filters |  |
|  |  | Replace hydraulic reservoir breather |  |
|  |  | 1500 Hours |  |
|  |  | Replace fan and drive belt |  |
|  |  | 2000 Hours |  |
|  |  | Clean pilot line filter |  |
|  |  | Change swing reduction unit oil |  |
|  |  | Change travel reduction unit oil |  |
|  |  | Change engine coolant |  |
|  |  | 3600 Hours |  |
|  |  | Replace DEF/ADBlue supply module filter |  |
|  |  | 5000 Hours |  |
|  |  | Change hydraulic oil |  |
|  |  | As Required |  |
|  |  | Check lights |  |
|  |  | Check batteries |  |
| Service  Technicians: | | | Machine Hours: |